CMSIS-Driver: NAND Bus Modes

| CMSIS-Driver Version 2.6.0 Peripheral Interface for Middleware and Application Code

- Main Page
- Usage and Description
- Reference

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Macros
NAND Bus Modes
NAND Control Codes

Specify bus mode of the NAND interface. More...

## Macros
#define | ARM_NAND_BUS_SDR (0x00UL << ARM_NAND_BUS_INTERFACE_Pos)
| Data Interface: SDR (Single Data Rate) - Traditional interface (default) More...
#define | ARM_NAND_BUS_DDR (0x01UL << ARM_NAND_BUS_INTERFACE_Pos)
| Data Interface: NV-DDR (Double Data Rate) More...
#define | ARM_NAND_BUS_DDR2 (0x02UL << ARM_NAND_BUS_INTERFACE_Pos)
| Data Interface: NV-DDR2 (Double Data Rate) More...
#define | ARM_NAND_BUS_TIMING_MODE_0 (0x00UL << ARM_NAND_BUS_TIMING_MODE_Pos)
| Timing Mode 0 (default) More...
#define | ARM_NAND_BUS_TIMING_MODE_1 (0x01UL << ARM_NAND_BUS_TIMING_MODE_Pos)
| Timing Mode 1. More...
#define | ARM_NAND_BUS_TIMING_MODE_2 (0x02UL << ARM_NAND_BUS_TIMING_MODE_Pos)
| Timing Mode 2. More...
#define | ARM_NAND_BUS_TIMING_MODE_3 (0x03UL << ARM_NAND_BUS_TIMING_MODE_Pos)
| Timing Mode 3. More...
#define | ARM_NAND_BUS_TIMING_MODE_4 (0x04UL << ARM_NAND_BUS_TIMING_MODE_Pos)
| Timing Mode 4 (SDR EDO capable) More...
#define | ARM_NAND_BUS_TIMING_MODE_5 (0x05UL << ARM_NAND_BUS_TIMING_MODE_Pos)
| Timing Mode 5 (SDR EDO capable) More...
#define | ARM_NAND_BUS_TIMING_MODE_6 (0x06UL << ARM_NAND_BUS_TIMING_MODE_Pos)
| Timing Mode 6 (NV-DDR2 only) More...
#define | ARM_NAND_BUS_TIMING_MODE_7 (0x07UL << ARM_NAND_BUS_TIMING_MODE_Pos)
| Timing Mode 7 (NV-DDR2 only) More...
#define | ARM_NAND_BUS_DDR2_DO_WCYC_0 (0x00UL << ARM_NAND_BUS_DDR2_DO_WCYC_Pos)
| DDR2 Data Output Warm-up cycles: 0 (default) More...
#define | ARM_NAND_BUS_DDR2_DO_WCYC_1 (0x01UL << ARM_NAND_BUS_DDR2_DO_WCYC_Pos)
| DDR2 Data Output Warm-up cycles: 1. More...
#define | ARM_NAND_BUS_DDR2_DO_WCYC_2 (0x02UL << ARM_NAND_BUS_DDR2_DO_WCYC_Pos)
| DDR2 Data Output Warm-up cycles: 2. More...
#define | ARM_NAND_BUS_DDR2_DO_WCYC_4 (0x03UL << ARM_NAND_BUS_DDR2_DO_WCYC_Pos)
| DDR2 Data Output Warm-up cycles: 4. More...
#define | ARM_NAND_BUS_DDR2_DI_WCYC_0 (0x00UL << ARM_NAND_BUS_DDR2_DI_WCYC_Pos)
| DDR2 Data Input Warm-up cycles: 0 (default) More...
#define | ARM_NAND_BUS_DDR2_DI_WCYC_1 (0x01UL << ARM_NAND_BUS_DDR2_DI_WCYC_Pos)
| DDR2 Data Input Warm-up cycles: 1. More...
#define | ARM_NAND_BUS_DDR2_DI_WCYC_2 (0x02UL << ARM_NAND_BUS_DDR2_DI_WCYC_Pos)
| DDR2 Data Input Warm-up cycles: 2. More...
#define | ARM_NAND_BUS_DDR2_DI_WCYC_4 (0x03UL << ARM_NAND_BUS_DDR2_DI_WCYC_Pos)
| DDR2 Data Input Warm-up cycles: 4. More...
#define | ARM_NAND_BUS_DDR2_VEN (1UL << 16)
| DDR2 Enable external VREFQ as reference. More...
#define | ARM_NAND_BUS_DDR2_CMPD (1UL << 17)
| DDR2 Enable complementary DQS (DQS_c) signal. More...
#define | ARM_NAND_BUS_DDR2_CMPR (1UL << 18)
| DDR2 Enable complementary RE_n (RE_c) signal. More...

## Description

Specify bus mode of the NAND interface.

The defines can be used in the function ARM_NAND_Control for the parameter arg and with the ARM_NAND_BUS_MODE as the control code.

## Macro Definition Documentation

#define ARM_NAND_BUS_SDR (0x00UL << ARM_NAND_BUS_INTERFACE_Pos)

Data Interface: SDR (Single Data Rate) - Traditional interface (default)

#define ARM_NAND_BUS_DDR (0x01UL << ARM_NAND_BUS_INTERFACE_Pos)

Data Interface: NV-DDR (Double Data Rate)

#define ARM_NAND_BUS_DDR2 (0x02UL << ARM_NAND_BUS_INTERFACE_Pos)

Data Interface: NV-DDR2 (Double Data Rate)

#define ARM_NAND_BUS_TIMING_MODE_0 (0x00UL << ARM_NAND_BUS_TIMING_MODE_Pos)

Timing Mode 0 (default)

#define ARM_NAND_BUS_TIMING_MODE_1 (0x01UL << ARM_NAND_BUS_TIMING_MODE_Pos)

Timing Mode 1.

#define ARM_NAND_BUS_TIMING_MODE_2 (0x02UL << ARM_NAND_BUS_TIMING_MODE_Pos)

Timing Mode 2.

#define ARM_NAND_BUS_TIMING_MODE_3 (0x03UL << ARM_NAND_BUS_TIMING_MODE_Pos)

Timing Mode 3.

#define ARM_NAND_BUS_TIMING_MODE_4 (0x04UL << ARM_NAND_BUS_TIMING_MODE_Pos)

Timing Mode 4 (SDR EDO capable)

#define ARM_NAND_BUS_TIMING_MODE_5 (0x05UL << ARM_NAND_BUS_TIMING_MODE_Pos)

Timing Mode 5 (SDR EDO capable)

#define ARM_NAND_BUS_TIMING_MODE_6 (0x06UL << ARM_NAND_BUS_TIMING_MODE_Pos)

Timing Mode 6 (NV-DDR2 only)

#define ARM_NAND_BUS_TIMING_MODE_7 (0x07UL << ARM_NAND_BUS_TIMING_MODE_Pos)

Timing Mode 7 (NV-DDR2 only)

#define ARM_NAND_BUS_DDR2_DO_WCYC_0 (0x00UL << ARM_NAND_BUS_DDR2_DO_WCYC_Pos)

DDR2 Data Output Warm-up cycles: 0 (default)

#define ARM_NAND_BUS_DDR2_DO_WCYC_1 (0x01UL << ARM_NAND_BUS_DDR2_DO_WCYC_Pos)

DDR2 Data Output Warm-up cycles: 1.

#define ARM_NAND_BUS_DDR2_DO_WCYC_2 (0x02UL << ARM_NAND_BUS_DDR2_DO_WCYC_Pos)

DDR2 Data Output Warm-up cycles: 2.

#define ARM_NAND_BUS_DDR2_DO_WCYC_4 (0x03UL << ARM_NAND_BUS_DDR2_DO_WCYC_Pos)

DDR2 Data Output Warm-up cycles: 4.

#define ARM_NAND_BUS_DDR2_DI_WCYC_0 (0x00UL << ARM_NAND_BUS_DDR2_DI_WCYC_Pos)

DDR2 Data Input Warm-up cycles: 0 (default)

#define ARM_NAND_BUS_DDR2_DI_WCYC_1 (0x01UL << ARM_NAND_BUS_DDR2_DI_WCYC_Pos)

DDR2 Data Input Warm-up cycles: 1.

#define ARM_NAND_BUS_DDR2_DI_WCYC_2 (0x02UL << ARM_NAND_BUS_DDR2_DI_WCYC_Pos)

DDR2 Data Input Warm-up cycles: 2.

#define ARM_NAND_BUS_DDR2_DI_WCYC_4 (0x03UL << ARM_NAND_BUS_DDR2_DI_WCYC_Pos)

DDR2 Data Input Warm-up cycles: 4.

#define ARM_NAND_BUS_DDR2_VEN (1UL << 16)

DDR2 Enable external VREFQ as reference.

#define ARM_NAND_BUS_DDR2_CMPD (1UL << 17)

DDR2 Enable complementary DQS (DQS_c) signal.

#define ARM_NAND_BUS_DDR2_CMPR (1UL << 18)

DDR2 Enable complementary RE_n (RE_c) signal.