CMSIS-Driver: I2C Events

| CMSIS-Driver Version 2.6.0 Peripheral Interface for Middleware and Application Code

- Main Page
- Usage and Description
- Reference

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Macros
I2C Events
I2C Interface

The I2C driver generates call back events that are notified via the function ARM_I2C_SignalEvent. More...

## Macros
#define | ARM_I2C_EVENT_TRANSFER_DONE (1UL << 0)
| Master/Slave Transmit/Receive finished. More...
#define | ARM_I2C_EVENT_TRANSFER_INCOMPLETE (1UL << 1)
| Master/Slave Transmit/Receive incomplete transfer. More...
#define | ARM_I2C_EVENT_SLAVE_TRANSMIT (1UL << 2)
| Addressed as Slave Transmitter but transmit operation is not set. More...
#define | ARM_I2C_EVENT_SLAVE_RECEIVE (1UL << 3)
| Addressed as Slave Receiver but receive operation is not set. More...
#define | ARM_I2C_EVENT_ADDRESS_NACK (1UL << 4)
| Address not acknowledged from Slave. More...
#define | ARM_I2C_EVENT_GENERAL_CALL (1UL << 5)
| Slave addressed with general call address. More...
#define | ARM_I2C_EVENT_ARBITRATION_LOST (1UL << 6)
| Master lost arbitration. More...
#define | ARM_I2C_EVENT_BUS_ERROR (1UL << 7)
| Bus error detected (START/STOP at illegal position) More...
#define | ARM_I2C_EVENT_BUS_CLEAR (1UL << 8)
| Bus clear finished. More...

## Description

The I2C driver generates call back events that are notified via the function ARM_I2C_SignalEvent.

This section provides the event values for the ARM_I2C_SignalEvent callback function.

The following call back notification events are generated:

## Macro Definition Documentation

#define ARM_I2C_EVENT_TRANSFER_DONE (1UL << 0)

Master/Slave Transmit/Receive finished.

#define ARM_I2C_EVENT_TRANSFER_INCOMPLETE (1UL << 1)

Master/Slave Transmit/Receive incomplete transfer.

#define ARM_I2C_EVENT_SLAVE_TRANSMIT (1UL << 2)

Addressed as Slave Transmitter but transmit operation is not set.

#define ARM_I2C_EVENT_SLAVE_RECEIVE (1UL << 3)

Addressed as Slave Receiver but receive operation is not set.

#define ARM_I2C_EVENT_ADDRESS_NACK (1UL << 4)

Address not acknowledged from Slave.

#define ARM_I2C_EVENT_GENERAL_CALL (1UL << 5)

Slave addressed with general call address.

#define ARM_I2C_EVENT_ARBITRATION_LOST (1UL << 6)

Master lost arbitration.

#define ARM_I2C_EVENT_BUS_ERROR (1UL << 7)

Bus error detected (START/STOP at illegal position)

#define ARM_I2C_EVENT_BUS_CLEAR (1UL << 8)

Bus clear finished.