CMSIS-DSP: Complex Magnitude Squared

| CMSIS-DSP Version 1.5.2 CMSIS DSP Software Library

- Main Page
- Usage and Description
- Reference

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Functions
Complex Magnitude Squared
Complex Math Functions

## Functions
void | arm_cmplx_mag_squared_f32 (float32_t *pSrc, float32_t *pDst, uint32_t numSamples)
| Floating-point complex magnitude squared. More...
void | arm_cmplx_mag_squared_q15 (q15_t *pSrc, q15_t *pDst, uint32_t numSamples)
| Q15 complex magnitude squared. More...
void | arm_cmplx_mag_squared_q31 (q31_t *pSrc, q31_t *pDst, uint32_t numSamples)
| Q31 complex magnitude squared. More...

## Description

Computes the magnitude squared of the elements of a complex data vector.

The `pSrc` points to the source data and `pDst` points to the where the result should be written. `numSamples` specifies the number of complex samples in the input array and the data is stored in an interleaved fashion (real, imag, real, imag, ...). The input array has a total of `2*numSamples` values; the output array has a total of `numSamples` values.

The underlying algorithm is used:

    for(n=0; n<numSamples; n++) {
        pDst[n] = pSrc[(2*n)+0]^2 + pSrc[(2*n)+1]^2;
    }

There are separate functions for floating-point, Q15, and Q31 data types.

## Function Documentation

void arm_cmplx_mag_squared_f32 | ( | float32_t * | pSrc,
|  | float32_t * | pDst,
|  | uint32_t | numSamples
| ) |  |

Parameters

  [in] | *pSrc | points to the complex input vector
  [out] | *pDst | points to the real output vector
  [in] | numSamples | number of complex samples in the input vector

Returns
  none.

void arm_cmplx_mag_squared_q15 | ( | q15_t * | pSrc,
|  | q15_t * | pDst,
|  | uint32_t | numSamples
| ) |  |

Parameters

  *pSrc | points to the complex input vector
  *pDst | points to the real output vector
  numSamples | number of complex samples in the input vector

Returns
  none.

Scaling and Overflow Behavior:

  The function implements 1.15 by 1.15 multiplications and finally output is converted into 3.13 format.

References __SIMD32, and __SMUAD().

void arm_cmplx_mag_squared_q31 | ( | q31_t * | pSrc,
|  | q31_t * | pDst,
|  | uint32_t | numSamples
| ) |  |

Parameters

  *pSrc | points to the complex input vector
  *pDst | points to the real output vector
  numSamples | number of complex samples in the input vector

Returns
  none.

Scaling and Overflow Behavior:

  The function implements 1.31 by 1.31 multiplications and finally output is converted into 3.29 format. Input down scaling is not required.