CMSIS-DAP: Reference

| CMSIS-DAP Version 2.0.0 Interface Firmware for CoreSight Debug Access Port

- Main Page
- Usage and Description
- Reference

All Functions Groups Pages
Reference
Here is a list of all modules:
[detail level 1 2 3]

Firmware Configuration | CMSIS-DAP is designed for Debug Units with Cortex-M microcontroller
Debug Unit Processor | CMSIS-DAP Firmware runs on Debug Units with a Cortex-M microcontroller
Configure I/O Ports and Debug Unit | DAP_config.h configures I/O ports and Debug Unit hardware parameters
CMSIS-DAP Debug Unit Information | Provides definitions about the hardware and configuration of the Debug Unit
CMSIS-DAP Hardware I/O Pin Access | Standard I/O Pins of the CMSIS-DAP Hardware Debug Port support standard JTAG mode and Serial Wire Debug (SWD) mode
CMSIS-DAP Hardware Status LEDs | CMSIS-DAP Hardware may provide LEDs that indicate the status of the CMSIS-DAP Debug Unit
CMSIS-DAP Timestamp | Access function for Test Domain Timer
CMSIS-DAP Initialization | CMSIS-DAP Hardware I/O and LED Pins are initialized with the function DAP_SETUP
Configure USB Peripheral | CMSIS-DAP Firmware communicates via an USB interface to host computer
Flash Program Firmware | The CMSIS-DAP Firmware is programmed into Flash ROM of a Debug Unit
Connect SWO Trace | Optional you may add a CMSIS-Driver USART to interface to SWO
Validate Debug Unit | A CMSIS-DAP conforming Debug Unit must be validated
CMSIS-DAP Commands | Commands between Debug Unit and host computer
General Commands | Information and Control commands for the CMSIS-DAP Debug Unit
DAP_Info | Get Information about CMSIS-DAP Debug Unit
DAP_HostStatus | Sent status information of the debugger to Debug Unit
DAP_Connect | Connect to Device and selected DAP mode
DAP_Disconnect | Disconnect from active Debug Port
DAP_WriteABORT | Write ABORT Register
DAP_Delay | Wait for specified delay
DAP_ResetTarget | Reset Target with Device specific sequence
Common SWD/JTAG Commands | Set SWD/JTAG clock and control/monitor SWD/JTAG I/O pins
DAP_SWJ_Pins | Control and monitor SWD/JTAG Pins
DAP_SWJ_Clock | Select SWD/JTAG Clock
DAP_SWJ_Sequence | Generate SWJ sequence SWDIO/TMS @SWCLK/TCK
SWD Commands | Configure the parameters for SWD mode
DAP_SWD_Configure | Configure SWD Protocol
DAP_SWD_Sequence | Generate SWD sequence and output on SWDIO or capture input from SWDIO data
SWO Commands | Configure the parameters for SWO mode
DAP_SWO_Transport | Set SWO transport mode
DAP_SWO_Mode | Set SWO capture mode
DAP_SWO_Baudrate | Set SWO baudrate
DAP_SWO_Control | Control SWO trace data capture
DAP_SWO_Status | Read SWO trace status
DAP_SWO_ExtendedStatus | Read SWO trace extended status
DAP_SWO_Data | Read SWO trace data
JTAG Commands | Detect and configure the JTAG device chain
DAP_JTAG_Sequence | Generate JTAG sequence TMS, TDI and capture TDO
DAP_JTAG_Configure | Configure JTAG Chain
DAP_JTAG_IDCODE | Read JTAG IDCODE
Transfer Commands | Read and Writes to CoreSight registers
DAP_TransferConfigure | Configure Transfers
DAP_Transfer | Read/write single and multiple registers
DAP_TransferBlock | Read/Write a block of data from/to a single register
DAP_TransferAbort | Abort current Transfer
Atomic Commands | Execute atomic commands
DAP_ExecuteCommands | Execute multiple DAP commands from a single packet
DAP_QueueCommands | Queue multiple DAP commands provided in a multiple packets
Response Status | Status Information in Response Data
CMSIS-DAP Vendor Commands | Extend CMSIS-DAP Firmware with commands